<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<!--Created by TARGET 3001! Version: 18.7.0.62-->
<!--DateTime: 2017.02.27 16:54:34-->
<eagle version="7.3.0">
	<drawing>
		<board>
			<plain>
				<wire x1="-15.4" y1="-10" x2="-15.4" y2="10" width="0.3" layer="20"/>
				<wire x1="25.6" y1="-10" x2="-15.4" y2="-10" width="0.3" layer="20"/>
				<wire x1="25.6" y1="-10" x2="25.6" y2="10" width="0.3" layer="20"/>
				<wire x1="25.6" y1="10" x2="-15.4" y2="10" width="0.3" layer="20"/>
				<text>Rev</text>
			</plain>
			<libraries>
				<library name="TARGET3001!_V18.7.0.62">
					<packages>
						<package name="SSOP28_0">
						</package>
						<package name="SOIC8_WB3,9_P1,27_1">
						</package>
						<package name="SL-MTA/2.54/4POL_2">
						</package>
						<package name="Assmann_A-USBS-B_3">
						</package>
						<package name="SOT23/3_5">
						</package>
						<package name="SOT23/3_6">
						</package>
						<package name="1206_7">
						</package>
						<package name="SMD_R9X9_ELKO_8">
						</package>
						<package name="1206_11">
						</package>
						<package name="1206_13">
						</package>
						<package name="SOD123_18">
						</package>
						<package name="SOD123_21">
						</package>
						<package name="1206_27">
						</package>
						<package name="1206_28">
						</package>
						<package name="1206_45">
						</package>
						<package name="PLCC2_46">
						</package>
						<package name="PLCC2_47">
						</package>
						<package name="1206_50">
						</package>
						<package name="1206_51">
						</package>
						<package name="PLCC2_55">
						</package>
						<package name="PLCC2_56">
						</package>
						<package name="PLCC2_57">
						</package>
						<package name="1206_60">
						</package>
						<package name="1206_63">
						</package>
						<package name="1206_64">
						</package>
						<package name="D5R2,54_ELKO_65">
						</package>
						<package name="1206_66">
						</package>
						<package name="1206_72">
						</package>
						<package name="0805_75">
						</package>
					</packages>
				</library>
			</libraries>
			<attributes/>
			<variantdefs/>
			<elements>
				<element name="IC1" library="TARGET3001!_V18.7.0.62" package="SSOP28_0" value="FT232RL">
					<attribute name="NAME"/>
				</element>
				<element name="IC3" library="TARGET3001!_V18.7.0.62" package="SOIC8_WB3,9_P1,27_1" value="MCP2025-500E/SN">
					<attribute name="NAME"/>
				</element>
				<element name="K2" library="TARGET3001!_V18.7.0.62" package="SL-MTA/2.54/4POL_2" value="640456-4"/>
				<element name="K3" library="TARGET3001!_V18.7.0.62" package="Assmann_A-USBS-B_3" value="A-USBS-B"/>
				<element name="D1" library="TARGET3001!_V18.7.0.62" package="SOT23/3_5" value="39V">
					<attribute name="VALUE"/>
				</element>
				<element name="D2" library="TARGET3001!_V18.7.0.62" package="SOT23/3_6" value="39V">
					<attribute name="VALUE"/>
				</element>
				<element name="C7" library="TARGET3001!_V18.7.0.62" package="1206_7" value="10µF">
					<attribute name="VALUE"/>
				</element>
				<element name="C8" library="TARGET3001!_V18.7.0.62" package="SMD_R9X9_ELKO_8" value="100µF">
					<attribute name="VALUE"/>
				</element>
				<element name="C9" library="TARGET3001!_V18.7.0.62" package="1206_11" value="100nF">
					<attribute name="VALUE"/>
				</element>
				<element name="C10" library="TARGET3001!_V18.7.0.62" package="1206_13" value="100nF">
					<attribute name="VALUE"/>
				</element>
				<element name="D4" library="TARGET3001!_V18.7.0.62" package="SOD123_18" value="1N4148W">
					<attribute name="NAME"/>
				</element>
				<element name="D5" library="TARGET3001!_V18.7.0.62" package="SOD123_21" value="1N4148W">
					<attribute name="NAME"/>
				</element>
				<element name="R23" library="TARGET3001!_V18.7.0.62" package="1206_27" value="1M">
					<attribute name="VALUE"/>
				</element>
				<element name="C12" library="TARGET3001!_V18.7.0.62" package="1206_28" value="4,7nF">
					<attribute name="VALUE"/>
				</element>
				<element name="C1" library="TARGET3001!_V18.7.0.62" package="1206_45" value="100nF">
					<attribute name="VALUE"/>
				</element>
				<element name="D3" library="TARGET3001!_V18.7.0.62" package="PLCC2_46" value="LS T67K">
					<attribute name="NAME"/>
				</element>
				<element name="D6" library="TARGET3001!_V18.7.0.62" package="PLCC2_47" value="LS T67K">
					<attribute name="NAME"/>
				</element>
				<element name="R1" library="TARGET3001!_V18.7.0.62" package="1206_50" value="150">
					<attribute name="VALUE"/>
				</element>
				<element name="R3" library="TARGET3001!_V18.7.0.62" package="1206_51" value="150">
					<attribute name="VALUE"/>
				</element>
				<element name="D7" library="TARGET3001!_V18.7.0.62" package="PLCC2_55" value="LG T67K">
					<attribute name="NAME"/>
				</element>
				<element name="D8" library="TARGET3001!_V18.7.0.62" package="PLCC2_56" value="LY T67K">
					<attribute name="NAME"/>
				</element>
				<element name="D9" library="TARGET3001!_V18.7.0.62" package="PLCC2_57" value="LY T67K">
					<attribute name="NAME"/>
				</element>
				<element name="R4" library="TARGET3001!_V18.7.0.62" package="1206_60" value="220">
					<attribute name="VALUE"/>
				</element>
				<element name="R5" library="TARGET3001!_V18.7.0.62" package="1206_63" value="330">
					<attribute name="VALUE"/>
				</element>
				<element name="R6" library="TARGET3001!_V18.7.0.62" package="1206_64" value="330">
					<attribute name="VALUE"/>
				</element>
				<element name="C16" library="TARGET3001!_V18.7.0.62" package="D5R2,54_ELKO_65" value="4,7µF">
					<attribute name="VALUE"/>
				</element>
				<element name="C2" library="TARGET3001!_V18.7.0.62" package="1206_66" value="100nF">
					<attribute name="VALUE"/>
				</element>
				<element name="R7" library="TARGET3001!_V18.7.0.62" package="1206_72" value="100K">
					<attribute name="VALUE"/>
				</element>
				<element name="J1" library="TARGET3001!_V18.7.0.62" package="0805_75" value="R_SMD_0-OHM_0805"/>
			</elements>
			<signals>
				<signal name="LIN">
					<contactref element="IC3" pad="4"/>
					<contactref element="K2" pad="4"/>
					<contactref element="D2" pad="3"/>
				</signal>
				<signal name="GND">
					<contactref element="IC1" pad="7"/>
					<contactref element="IC1" pad="26"/>
					<contactref element="IC1" pad="25"/>
					<contactref element="IC1" pad="21"/>
					<contactref element="IC1" pad="18"/>
					<contactref element="IC3" pad="3"/>
					<contactref element="K2" pad="1"/>
					<contactref element="K3" pad="4"/>
					<contactref element="D1" pad="1"/>
					<contactref element="D2" pad="1"/>
					<contactref element="C7" pad="2"/>
					<contactref element="C8" pad="2"/>
					<contactref element="C9" pad="2"/>
					<contactref element="C10" pad="2"/>
					<contactref element="R23" pad="1"/>
					<contactref element="C12" pad="1"/>
					<contactref element="C1" pad="2"/>
					<contactref element="D7" pad="2"/>
					<contactref element="D8" pad="2"/>
					<contactref element="D9" pad="2"/>
					<contactref element="C16" pad="2"/>
					<contactref element="C2" pad="1"/>
				</signal>
				<signal name="RXD">
					<contactref element="IC1" pad="5"/>
					<contactref element="IC3" pad="5"/>
				</signal>
				<signal name="TXD">
					<contactref element="IC1" pad="1"/>
					<contactref element="IC3" pad="6"/>
				</signal>
				<signal name="D+">
					<contactref element="IC1" pad="15"/>
					<contactref element="K3" pad="3"/>
				</signal>
				<signal name="+12V">
					<contactref element="IC3" pad="1"/>
					<contactref element="K2" pad="2"/>
					<contactref element="D1" pad="3"/>
					<contactref element="C8" pad="1"/>
					<contactref element="C9" pad="1"/>
				</signal>
				<signal name="+5V">
					<contactref element="IC3" pad="8"/>
					<contactref element="C7" pad="1"/>
					<contactref element="C10" pad="1"/>
					<contactref element="D5" pad="1"/>
					<contactref element="R5" pad="1"/>
				</signal>
				<signal name="VCC_USB">
					<contactref element="K3" pad="1"/>
					<contactref element="D4" pad="1"/>
					<contactref element="R6" pad="1"/>
				</signal>
				<signal name="|RESET|">
					<contactref element="IC3" pad="7"/>
					<contactref element="J1" pad="1"/>
				</signal>
				<signal name="RTS#">
					<contactref element="IC1" pad="3"/>
					<contactref element="IC3" pad="2"/>
				</signal>
				<signal name="VCC_FT">
					<contactref element="IC1" pad="4"/>
					<contactref element="IC1" pad="20"/>
					<contactref element="D4" pad="2"/>
					<contactref element="D5" pad="2"/>
					<contactref element="C1" pad="1"/>
					<contactref element="R1" pad="1"/>
					<contactref element="R3" pad="1"/>
					<contactref element="R4" pad="1"/>
					<contactref element="C16" pad="1"/>
					<contactref element="R7" pad="1"/>
				</signal>
				<signal name="D-">
					<contactref element="IC1" pad="16"/>
					<contactref element="K3" pad="2"/>
				</signal>
				<signal name="Shield">
					<contactref element="K3" pad="5"/>
					<contactref element="R23" pad="2"/>
					<contactref element="C12" pad="2"/>
				</signal>
				<signal name="RXLED">
					<contactref element="IC1" pad="22"/>
					<contactref element="D6" pad="2"/>
				</signal>
				<signal name="TXLED">
					<contactref element="IC1" pad="23"/>
					<contactref element="D3" pad="2"/>
				</signal>
				<signal name="3V3OUT">
					<contactref element="IC1" pad="17"/>
					<contactref element="C2" pad="2"/>
				</signal>
				<signal name="RESET#">
					<contactref element="IC1" pad="19"/>
					<contactref element="R7" pad="2"/>
					<contactref element="J1" pad="2"/>
				</signal>
				<signal name="R_Vcc_FT">
					<contactref element="D7" pad="1"/>
					<contactref element="R4" pad="2"/>
				</signal>
				<signal name="R_5V">
					<contactref element="D8" pad="1"/>
					<contactref element="R5" pad="2"/>
				</signal>
				<signal name="R_Vcc_USB">
					<contactref element="D9" pad="1"/>
					<contactref element="R6" pad="2"/>
				</signal>
				<signal name="R_TX">
					<contactref element="D3" pad="1"/>
					<contactref element="R1" pad="2"/>
				</signal>
				<signal name="R_RX">
					<contactref element="D6" pad="1"/>
					<contactref element="R3" pad="2"/>
				</signal>
				<signal name="AGND"/>
				<signal name="VBB"/>
				<signal name="VCC"/>
				<signal name="VCCIO"/>
				<signal name="VSS"/>
			</signals>
		</board>
	</drawing>
</eagle>
