[logging]
path=/var/log/lorabot.log

[lora]
type=Draginolora
pin_sspin=Pin06
pin_dio0=Pin07
pin_rst=Pin00
frequency=868100000
spreadingfactor=8
signalbandwith=125000
codingrate=6

;[lora]
;type=Ic880alora
;pin_sspin=Pin10
;pin_rst=Pin21
;spichan=Channel0
; Set Basic Frequencies
;frequency0=867500000
;frequency1=868500000
; Set Per Virtual Interface IF0-7 (Freq means the offset to the basic frequency)
;interface0enable=true
;interface0chain=1
;interface0frequency=-400000
;interface1enable=true
;interface1chain=1
;interface1frequency=-200000
;interface2enable=true
;interface2chain=1
;interface2frequency=0
;interface3enable=true
;interface3chain=0
;interface3frequency=-400000
;interface4enable=true
;interface4chain=0
;interface4frequency=-200000
;interface5enable=true
;interface5chain=0
;interface5frequency=0
;interface6enable=true
;interface6chain=0
;interface6frequency=200000
;interface7enable=true
;interface7chain=0
;interface7frequency=400000
; Virtual Interface IF8 Lora Interface
;interface8enable=false
;interface8chain=1
;interface8frequency=-200000
;lorabandwith=250000
;loraspreadingfactor=7
; Virtual Interface IF9 FSK Interface
;interface9enable=false
;interface9chain=1
;interface9frequency=300000
;fskbandwith=125000
;fskdatarate=50000