[logging]
path=/var/log/lorabot.log

;[lora]
;type=Draginolora
;pin_sspin=Pin06
;pin_dio0=Pin07
;pin_rst=Pin00
;frequency=868100000
;spreadingfactor=8
;signalbandwith=125000
;codingrate=6

[lora]
type=Ic880alora
pin_sspin=Pin10
pin_rst=Pin21
spichan=Channel0
; Set Basic Frequencies
frequency0=867125000
frequency1=868125000
; Set Per Virtual Interface IF0-7 (Freq means the offset to the basic frequency)
interface0enable=true
interface0chain=0
interface0frequency=-375000
interface1enable=true
interface1chain=0
interface1frequency=-125000
interface2enable=true
interface2chain=0
interface2frequency=125000
interface3enable=true
interface3chain=0
interface3frequency=375000
interface4enable=true
interface4chain=1
interface4frequency=-375000
interface5enable=true
interface5chain=1
interface5frequency=-125000
interface6enable=true
interface6chain=1
interface6frequency=125000
interface7enable=true
interface7chain=1
interface7frequency=375000
; Virtual Interface IF8 Lora Interface
interface8enable=false
interface8chain=1
interface8frequency=-200000
lorabandwith=250000
loraspreadingfactor=7
; Virtual Interface IF9 FSK Interface
interface9enable=false
interface9chain=1
interface9frequency=300000
fskbandwith=125000
fskdatarate=50000
